mBPS-d2s Battery Replacement Manual

CAUTION If circumstances allow, ask replacement to distributor or retail shop. Be careful not to overtighten screws. Please recycle your used batteries that have explosion risk

Remove eight Torx screws carefully

Remove the LED ribbon cable by pulling down

Remove the two connectors which are placed in front of the batteries by pulling down

Pry the battery packs off the back plate carefully by using tools such as straight razor

Remove residual tape on the back-plate

Remove backing on the two way tape from the new battery; center carefully on the board and make a little space between two batteries

Plug the battery terminals in, and then screw every plates to complete replacement